### uVision2 Project, (C) Keil Software
### Do not modify !

Target (Target 1), 0x0000 // Tools: 'MCS-51'

Group (Source Group 1)

File 1,1,<.\fw.c><fw.c> 0x0 
File 1,2,<.\dscr.a51><dscr.a51> 0x0 
File 1,4,<.\EZUSB.LIB><EZUSB.LIB> 0x434BE588 
File 1,3,<.\USBJmpTb.OBJ><USBJmpTb.OBJ> 0x0 
File 1,1,<.\interrupciones.c><interrupciones.c> 0x0 
File 1,1,<.\pedalera.c><pedalera.c> 0x0 
File 1,1,<.\I2C.c><I2C.c> 0x0 


Options 1,0,0  // Target 'Target 1'
 Device (EZ-USB FX2 (CY7C68XXX))
 Vendor (Cypress Semiconductor)
 Cpu (IRAM(0 - 0xFF) XRAM(0 - 0x3FF) CLOCK(48000000) MODDP2)
 FlashUt ()
 StupF ()
 FlashDR ()
 DevID ()
 Rgf (REG52.H)
 Mem ()
 C ()
 A ()
 RL ()
 OH ()
 DBC_IFX ()
 DBC_CMS ()
 DBC_AMS ()
 DBC_LMS ()
 UseEnv=1
 EnvBin (C:\Keil\C51\BIN\)
 EnvInc (c:\CYPRESS\USB\Target\Inc\;C:\Keil\C51\INC\)
 EnvLib (C:\Keil\C51\LIB\)
 EnvReg ()
 OrgReg ()
 TgStat=16
 OutDir (.\)
 OutName (InterfazPedalera)
 GenApp=1
 GenLib=0
 GenHex=1
 Debug=1
 Browse=0
 LstDir (.\)
 HexSel=0
 MG32K=0
 TGMORE=0
 RunUsr 0 1 <c:\cypress\usb\bin\hex2bix -i -f 0xC2 -o InterfazPedalera.hex.iic InterfazPedalera.hex>
 RunUsr 1 0 <>
 BrunUsr 0 0 <>
 BrunUsr 1 0 <>
 SVCSID <>
 MODEL5=0
 RTOS5=0
 ROMSZ5=2
 DHOLD5=0
 XHOLD5=0
 T51FL=304
 XT51FL=0
 CBANKS5=0
 XBANKS5=0
 RCB51 { 0,0,0,0,0,255,255,0,0 }
 RXB51 { 0,0,0,0,0,0,0,0,0 }
 OCM51 { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCR51 { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IRO51 { 0,0,0,0,0,0,0,0,0 }
 IRA51 { 0,0,0,0,0,0,1,0,0 }
 XRA51 { 0,0,0,0,0,0,4,0,0 }
 XRA512 { 0,0,0,0,0,0,0,0,0 }
 IROM512 { 0,0,0,0,0,0,0,0,0 }
 C51FL=21630224
 C51VA=0
 C51MSC ()
 C51DEF ()
 C51UDF ()
 INCC5 ()
 AX51FL=4
 AX51MSC ()
 AX51SET ()
 AX51RST ()
 INCA5 ()
 PropFld { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IncBld=1
 AlwaysBuild=0
 GenAsm=0
 AsmAsm=0
 PublicsOnly=0
 StopCode=3
 CustArgs ()
 LibMods ()
 BankNo=65535
 LX51FL=288
 LX51OVL ()
 LX51MSC ()
 LX51DWN ()
 LX51LFI ()
 LX51ASN ()
 LX51RES ()
 LX51CCL ()
 LX51UCL ()
 LX51CSC ()
 LX51UCS ()
 LX51COB (0x80-0x1FFF)
 LX51XDB (0x2000)
 LX51PDB ()
 LX51BIB ()
 LX51DAB ()
 LX51IDB ()
 LX51PRC ()
 LX51STK ()
 LX51COS ()
 LX51XDS ()
 LX51BIS ()
 LX51DAS ()
 LX51IDS ()
  OPTDL (S8051.DLL)()(DP51.DLL)(-pFX2)(S8051.DLL)()(TP51.DLL)(-pFX2)
  OPTDBG 49150,-1,()()()()()()()()()() (BIN\MON51.DLL)()()()
 FLASH1 { 1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 FLASH2 ()
 FLASH3 ("" ())
 FLASH4 ()
EndOpt

